High Speed Adjustment
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Remove the belt cover.  Turn on your Shopsmith and crank up the speed until the drive belt is 1/8" to 1/16" from the outside edge of the motor pulley, or until the high speed stop keeps you from turning it any further. 

Remove the control handle. (Watch out-the machine is running and the belts are exposed!)
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Use a small screwdriver to hold the set screw, then loosen the jam nut.

If the high speed stop engaged before the drive belt was [image: image3.jpg]


near the edge of the motor pulley, turn the set screw COUNTERCLOCKWISE and, at the same time, turn the worm shaft CLOCKWISE until the belt is between 1/8" and 1/16" from the outer edge of the pulley. Note the use of pads on the pliers-this is to protect the worm shaft. This is the Shopsmith recommended procedure.
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Turn off your Shopsmith. Re-tighten the jam nut. Press in and turn the speed dial until it reads "fast." 
