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Cabinet

by T Parks
There's a whole lot of storage space just waiting to be filled —
right under your Mark V1

T pywood cabinet s a perfect mate fo the Mark V. || makes
good seof he space underneaih i mashine, crestng a s
Drsing amount o sorage spaco o 1ols and accessories
‘Phoce casy.10-misplac 1ams Such as arors, moder kivos,
Sa blaces, and sandin diecs can b stred faadyio-use right
WTersou Can roach ihem, Evenarger Wark  Sccessorios Such
2516 inter and belt sandr Gan i Inios s cavinel

By mouving The bangsaw and Jgsaw on o cnasof e Mark V.
5 colgie of ackessorios on the op o e cabinet,and the res
onthainside of . ail th foms in e Ulimate Shop Accescory.
Packago. and the MarkV sel,can be stored n 12 scuare oo
Tt aboutine size ot awal i closet!

it piywiood sco0rding 1otho cuting digram win he help
of ancir person. e & pyiaod or earbide-pped Saw bisas
S5 woodn fonce axtonslon 1o greater Doaring Suriace and
s coneo for gt cuts

‘e il o pisces arocut,sotup tho dado packago o ctal
iadoes 112" ide by 1/5 Gsepor gides and assemdy. For ac-
Curacy, cut and Sant the i contoursq snds togather. Then orl
{he mobinting bot hojes I he ends and the iamp bars. Drl for
Goorknob screws as el

o may 05210 oy ons plece 1415 172 o an ke
S it S e

Dry assemble the cabinetusing bar olamps and checkthe il
of doore and shelves Mark or hinge morises: Measurs and cut
e Sluminum angla tock 10 15 1angthg and il scren noise i

Now cisassembie the cabinet Chisel i mordsas for 10
Pinges, Moun ha andia t0¢k 56 8ure o eave room 1 the
Godreio cioe,

Feclar he cabioe parts togeiher and fasten i screws
only Use o lue: Mount fhe door knobs, inges, and iiches
heldoore. The clps Under ne shalves hatprevent hem fom
ipping &nd spiing shauid ba mouec near ach selfs back
eae.

our the cabinet 0 he Undsraide of the Mark V. il L with .
essories an 0olsarrangad o S0l your personl ioads. At
e cabmet A, 1 1 doors I isca. Than ko all e
At cutof he Cabingtone st e, clsassembie  and apply
Gl to i o, reusing he Iy S6rews again 1o clamp ufie
Shegliesate Tham you can il he serow head counlerainks win
ot puty and Sppy the ish ofyour choice

"This cabinat car be modifed t ol on castrs 0 e sed a3 3
lowlevetwork suriace. You can 80 g modlicatons 1 hold
1he cyter ollecto gefeciore rom e Shopsmit projectplan,
e Shapsimin Sawdust Colecion Syster
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NOTE: SHELF SPACING 3" EXCEPT
WHERE NOTED
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SHELF_MOUNTING DETAL

Bill of Materials / NOTE: ONE DOOR
(finished dimensions in inches) NOT SHC
A Top
andBotom (2)  112x 18 xd6-172
& Ends(2) iz ez
© Fariion 1120 10% 15304

D Back 172 151/2 12314
EDoors(a)  12xi15i2x 16112
F Door 112315112 12.3/4
G Braces(z  1/2x2-1/2xd617a
H Shelves3) 123 14-172x 12.3/4
3 shai 112X 12:3/4%7-3/4
K Sneir 2411233
L Clamobars (2) 1722112 15:1/2

Hardware
10 3" Toninges with screws
13178 12 1/2 Auminum angle
30 48 172" Panhead sheel metal scroms.
S Knobe

42 B 1172 Uty srens.
2 "Witro retiner lps.

CABINET ASSEMBLY
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