
NEVER ADJUST SPEED WITH POWER OFF!

BEFORE POWER ON:
1. CHECK SPEED
2. INSPECT: ARE THESE LOCKED? (clockwise)
a) Quill

b) Headstock

c) Carriage

d) Table Lift 

e) Table Tilt

f) Vertical Lock Screw when going to drill press mode. 
note: DO release prior to lowering to horizontal.
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