Shopsmith Tool List & Maintenance Schedule





         Annual = January
       Quarterly = January/April/July/October

	Tool
	Serial #
	Size(s)
	Maintenance Schedule
	Months

	
	
	
	
	1
	3
	12

	Headstock (2)
	
	10” Circular saw blade

½” Jacob Chuck 
	Clean thoroughly including blowing out headstock.

Lubricate (oil) driveshaft and idler shaft;   Wax way tubes, bench tubes, table, support tubes, quill, miter gauge, rip fence, extension tables and accessory mounting holes;  Check alignment and adjustment of the table, table inserts, table stops, trunnion stops, miter gauge, rip fence, extension tables and lath centers;  Check the tension on the Poly V-belt.

Lubricate sheaves and headstock lock.
	X
	X
	X

	Air Compressor
	
	0-90 PSI
	Replace air filter
	
	
	X

	Bandsaw - 11”
	
	72” Blade
	Lubricate (graphite) trunnions, blade tension screw, blade guidepost and blade guide adjusting screws.  Wax table and check table alignment.

Lubricate (grease) the needle bearings.  Check all guide blocks, roller bearings, tires and needle bearings for wear.
	
	X
	X

	Belt Sander – 6”
	
	6” X 48” Belt
	Wax backup plate and table.

Wax trunnion guides.
	
	X


	X

	Disk Sander – 12”
	NA
	12” Disk
	NA
	
	
	

	Drum Sander – 2”
	NA
	2” x ½”, ¾”, 1”, 1 ½”
	NA
	
	
	

	Dust Collector
	
	1 ¼”, 2 ¼” Hoses
	NA
	
	
	

	Jigsaw – 18”

Sabersaw
	
	Sabersaw blade:  3 ⅛”

Jeweler’s blade:  5 ¼”

Jigsaw blade:  5 ¼”

Pattern files:  5 ¼”
	Lubricate (oil) pump seal, reface lower blade guide, wax table and check table alignment.

Replace oil, 3 oz, 10W.
	
	X
	X

	Jointer – 4”
	
	4” Blades
	Blow out jointer, inspect and hone knives, remove pitch, check wedge locking screws, and wax table. 

Dismantle jointer, remove impacted wood chips, wax machined surfaces, lubricate (graphite) adjustment shaft, tighten bearing housing bolts and check alignment.
	X
	
	X

	Maxi Clamp
	NA
	⅜” Threaded rod
	NA
	
	
	

	Mortising System
	NA
	¼”, ⅜”, ½” Chisels 
	NA
	
	
	

	Power Station
	
	NA
	Clean thoroughly.  Also wax the carriage holes and the carriage glide surface.  Lubrication:  only the motor needs lubricating.  You should oil the motor according to the directions on your motor label.  If your label is missing or unreadable, oil your motor after every fifty (50) hours of use with approximately 150 drops (1 Tsp.) of SAE 20.  Check that the setscrews of upper and lower pulleys are securely tightened.
	
	 X
	X

	Pro Planer – 12”
	
	12” Blades
	Blow out planer, inspect and hone knives, remove pitch, wax tie bars, cutterhead and table.

Dismantle planer, remove impacted wood chips, check synchronizing chain tension and roller pressure, lubricate (graphite) synchronizing chain, roller arm bushings, the threads of the mounting post and check alignment.
	X
	
	X

	Routing
	NA
	¼” Router bit
	NA
	
	
	

	Sharpening Guide
	NA
	3” Bench & 4” Lathe chisels
	NA
	
	
	

	Shaper Fence
	NA
	NA
	NA
	
	
	

	Tenon Jig
	NA
	NA
	NA
	
	
	


