	Power Station Settings for Bandsaw

	
	
	
	

	Blade Size
	Hardwood RPM
	Softwood RPM
	

	1/16”
	950          1-1/2
	1050         2
	

	1/8”
	950          1-1/2
	1050         2
	

	¼”
	850          1
	950          1-1/2
	

	½”
	850          1
	850          1
	

	5/8”
	850          1
	850          1
	

	
	
	
	

	Jointer set to the highest setting
	
	

	But, better to place to left of saw for higher speed
	
	

	
	
	
	


